85 WEST HIGHWAY M-115

BOON, MICHIGAN 49618

PHONE 231-775-9731

FAX 231-775-9732

WWW.WEXFORDCRC.ORG

HARRY HAGSTROM, CHAIRMAN HAROLD FALAN, VICE-CHARIMAN

DEAN JURIK, MEMBER

JIM LEGGETT, MEMBER

ROBERT HILTY, MEMBER

***WEXFORD COUNTY ROAD COMMISSION***

***OUR MISSION IS TO IMPROVE AND MAINTAIN A SAFE AND EFFICIENT ROAD SYSTEM***

BID PROPOSAL

Sealed bids will be received at the office of the Wexford County Road Commission, 85 W. M-115, Boon, Michigan 49618 until **2:30 p.m. Friday, January 27th, 2023** for

One (2) **Diamond C HDT82” x 24’ Tilt Deck Equipment Trailers**(or equivalent)

Specifications and bid sheets can be obtained at the above address or by visiting www.wexfordcrc.org.

All bids must be submitted in a sealed envelope bearing the name of bidder, item being bid, and clearly marked as a sealed bid.

The Wexford County Road Commission, in accordance with Title VI of the Civil Rights Act of 1964, 78 Stat. 252, 42 USC 2000d to 2000d-4 and Title 49, Code of Federal Regulations, Department of Federally-assisted programs of the Department of Transportation issued pursuant to such Act, hereby notifies all bidders that it will affirmatively insure that in any contract entered into pursuant to this advertisement, minority business enterprises will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of gender, disability, race, color, or national origin in consideration for an award.

The Board reserves the right to reject any or all bids, waive any defects, and to accept the bid which, in its opinion, is the most advantageous to the Road Commission.

WEXFORD COUNTY ROAD COMMISSION

Harry Hagstrom, Chairman

Harold Falan, Vice Chairman

Jim Leggett, Member

Dean Jurik, Member

Robert Hilty, Member

WEXFORD COUNTY ROAD COMMISSION (WCRC)

Two (2) **Diamond C HDT82” x 24’ Tilt Deck Equipment Trailers**

**Bid due @ 2:00 p.m. Friday, January 27th, 2023**

**85 W. M-115, Boon, MI 49618**

**231-775-9731**

This bid sheet must be used for submitting a bid for Two (2) **Diamond C HDT82” x 24’ Tilt Deck Equipment Trailers**, meeting specifications listed below. Please indicate “yes” if bid meets specification, or list the deviation from specification, for each item.

**Diamond C HDT82” x 24’ Tilt Deck Equipment Trailer, or equivalent.**

These specifications include furnishing and delivering of Two (2) **Diamond C HDT82” x 24’ Tilt Deck Equipment Trailer**. **To be delivered in 2023 unless otherwise agreed upon.**

The unit is to be complete per these specifications. Bidders may recommend options, indicating type and specifications for the options, as supplementary bids to be considered as part of the bid.

New equipment being bid per specifications on following pages:

Make: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Model: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Year: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

MINIMUM SPECIFICATIONS:

GVWR Specifications:

1. 210 Package or 20K GVWR

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Frame specifications:

1. Engineered beam frame of 8”x 15lb I-Beam tongue/frame design.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Cross-members must be 3” I-Beam on 12” centers. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
2. Frame painted red in color with exceptional pretreating process to increase frame longevity.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. No less than eight (8) D-Rings spaced evenly (four per side) the length of frame for load securement, painted to match trailer.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Axle Specifications:

1. Tandem (2) torsion style axles with electric drum brakes on both, rated at 10,000lbs each.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. Oil bath hubs.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Suspension Specifications:

1. Torsion style suspension.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Tire/Wheel Specifications:

1. Wheels are to be black in color, have a spare tire mount on the curb side of trailer as well as having a matching spare tire/wheel included in purchase of trailer.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. Tires must be matched to GVWR of trailer rating and to be no less than a 215/75R17.5 in size with a 16 ply rating.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Deck Specifications:

1. 8’ Stationary deck at front.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. 2” treated lumber floor.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

3. 3/16” teardrop, diamond plate weld on fenders painted to match frame.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Tilt Specifications:

1. Hydraulic dampening cylinder with valve control.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Coupler Specifications:

1. Must be a bumper pull style coupler with a 2-5/16 21,000LB rated system with break away.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Jack Specifications:

1. Minimum of one (1) 12,000 lb drop leg jack located in either the center of tongue or on road side of trailer.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Light Specifications:

1. Lights must meet all local and federal specifications as far as number of and placement.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. All lights on trailer must be LED.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Required Optional Accessories:

1. Trailer must have storage area in tongue of trailer WITH a lid painted to match trailer.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. Trailer must have a 2” rub rail constructed of 3/8” steel painted to match trailer the length of each side of the trailer and to include stake pockets.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

3. Trailer must have integrated fork holders on the trailer for skid steer forks.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

4. Must include at least one (1) 36” side step located on the road side.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

WARRANTY QUESTIONNAIRE:

Indicate month and/or miles of warranty on the listed components:

Trailer Frame Months\_\_\_\_\_\_\_ Provider\_\_\_\_\_\_\_\_\_\_\_

Axles (Hub to Hub) Months \_\_\_\_\_\_\_ Provider \_\_\_\_\_\_\_\_\_\_

Wheels Months\_\_\_\_\_\_\_\_ Provider\_\_\_\_\_\_\_\_\_\_\_

Tires Months\_\_\_\_\_\_\_\_ Provider\_\_\_\_\_\_\_\_\_\_\_

Jack Months\_\_\_\_\_\_\_\_ Provider\_\_\_\_\_\_\_\_\_\_\_

\*All warranty start-up dates to be when completed by vendor and road-ready at WCRC.

\*Machine trailer & optional components must be complete.

\*Machine must meet all Federal, State & local safety standards.

\*Successful bidder must furnish complete paper book or CD type illustrated parts, operator, electrical & service manuals, and line setting tickets at time of delivery.

\*Included in the above described manuals shall be engine and machine.

\*Diagnostic and minor repair training shall be provided for the WCRC shop staff at the WCRC facility.

\*Bidder must provide descriptive literature with their bid.

\*Bidder must indicate any deviations from specifications and mark yes or no at each item bid.

\*All bids must be submitted in a sealed envelope bearing the name of bidder, appropriately marked as to the item being bid, and marked as a sealed bid.

\*Price to be F.O.B. Wexford County Road Commission garage, 85 W. M-115, Boon, MI 49618

\*Tax Exemption certificate will be signed upon request.

Total bid price for new unit(s) according to above specifications:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Terms \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date of Delivery at Wexford County Road Commission \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Submitted by:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Company Name Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address Name (Typed or printed)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

City, State, Zip Title of person signing (typed or printed)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Telephone Date

Please contact Travis Smith, Fleet & Facilities Manager, at (616)862-3043, with any questions regarding these specifications.